The '''OPEN COM''' statement is used to access a computer's Serial port COM1 or COM2  address using an OPEN statement.



{{PageSyntax}}
: '''OPEN &quot;COMn:''' ''Speed'', ''Parity'', ''Bits'', ''Stopbit'', [''Options'']&quot; [FOR {[[RANDOM]]|[[BINARY]]|[[OUTPUT]]|[[INPUT (file mode)|INPUT]]}] AS #''P'' [LEN = ''bytesize'']


{{Parameters}}
* ''Speed'' (baud rate): 50, 150, 300, 600, 1200, 1800, 2400, '''9600''' (QB max), 19200 or '''115200''' ('''QB64''' max) maximum.
* ''Parity'': '''N''' (none), E (even), O (odd), S (space) or M (mark). Note: If 8 bits use parity N for numerical data!
* ''Bits'' = number of bits/byte: Valid numbers: 5, 6, 7 or '''8'''
* ''Stopbit'' = number of stop bits: Valid numbers: '''1''', 1.5 or 2
* Optional COM port ''Options'' (separated by commas):
::* ASC : [[ASCII]] byte mode. End of line = [[CHR$]](13). End of file = CHR$(26)
::* BIN : [[Binary]] byte mode. Default mode if ASC is not used(option not required).
:: ''Below ms is the timeout in milliseconds 1 to 65535. Zero ignores a timeout. Default without ms = 1000 :''
::* CD[ms] : Time until timeout of DCD (Carrier Detect) line in. CD0 ignores timeouts.
::* CS[ms] : Time until timeout of CTS (Clear to Send) line in. CS0 ignores timeouts.
::* DS[ms] : Time until timeout of DSR (Data Set Ready) line in. DS0 ignores timeouts.
::* OP[ms] : Time until data lines become active. If timeout then OPEN fails! OP0 ignores timeouts.
::* RB[b] : Size of receive buffer in bytes when used. Default when not used = 512 bytes
::* TB[b] : Size of transmit buffer in bytes when used. Default when not used = 512 bytes
::* RS  : Supress detection of Request to Send (RTS) line.


{{PageDescription}}
* '''If any optional CD, CS, DS or OP timeouts occur the OPEN will fail or port access will stop! Try 0 to ignore.'''		   
* '''QB64''' can open any [[COM(n)|COM''n'']] port number. Qbasic could only open COM1 or COM2, but 3 and 4 could be swapped.
* See Windows System '''Device Manager''' for COM port numbers and port addresses &amp;H3F8, &amp;H2F8, &amp;H3E8 and &amp;H2E8.
* Four commas are required after the Speed, Parity, Bits, and Stopbit, even if none of the Options are used.
* Other [[OPEN]] ''options'' are optional and in any order separated by commas within the OPEN command [[STRING|string]].(See list below)
* The optional FOR access ''mode'' can be [[OUTPUT]], [[INPUT (file mode)|INPUT]] or [[RANDOM]] (default mode when no FOR statement is used). 
* '''Currently, QB64 only supports [[OPEN]] FOR [[RANDOM]] access using the [[GET]]/[[PUT]] commands in [[BINARY|BIN]] mode!'''
* '''Use the BIN option listed below for [[BINARY]] byte mode port access!'''
* The [[LEN]] statement is also optional. The default record size is 512 bytes when not used.
* Use the [[LOC]](portnumber) function to determine that there is data in the receive buffer when the value is greater than 0.
* OPEN AS number can use a [[FREEFILE]] value. Numbers used by files already open '''cannot''' be used by OPEN COM!
* [[Keywords_currently_not_supported_by_QB64#Keywords_Not_Supported_in_Linux_or_MAC_OSX_versions|Keyword Not Supported in Linux or MAC versions]]


&lt;center&gt;'''Qbasic Description NOT Currently supported in QB64!'''&lt;/center&gt;
*[[INPUT (file mode)|INPUT]] mode can use [[INPUT (file statement)|INPUT #]] or [[INPUT$]]. [[OUTPUT]] mode can use [[PRINT (file statement)|PRINT #]] or [[PRINT USING (file statement)|PRINT #, USING]].  
*[[RANDOM]] or [[BINARY|BIN]] modes can use [[INPUT (file statement)|INPUT #]], [[INPUT$]], [[PRINT (file statement)|PRINT #]], [[GET]] or [[PUT]]. BIN cannot set a buffer size!
* Note: If random use [[LEN]] = to set size of random buffer(default LEN = 128). Use multiples of 128 for larger buffers.
* NOTE: NT or XP computers need a program like [http://www.beyondlogic.org/porttalk/porttalk.htm PortTalk] to access COM or other ports with Qbasic only!


''Example 1:'' Checking to see if a COM port exists. If the port does not exist Qbasic will cause a Windows access error! 
{{CodeStart}} '' ''
{{Cl|ON ERROR}} {{Cl|GOTO}} Handler 
FF = {{Cl|FREEFILE}}
comPort$ = &quot;COM1:&quot;                         'try a COM port number that does not exist
{{Cl|CONST}} comMode$ = &quot;9600,N,8,1,CS0,DS0&quot;      'Use 0 to avoid timeouts 
{{Cl|OPEN}} comPort$ + comMode$ {{Cl|FOR...NEXT|FOR}} {{Cl|RANDOM}} {{Cl|AS}} FF 
{{Cl|IF...THEN|IF}} errnum = 0 {{Cl|THEN}} {{Cl|PRINT}} &quot;COM exists!

K$ = {{Cl|INPUT$}}(1) 
{{Cl|END}} 

Handler: 
errnum = {{Cl|ERR}} 
{{Cl|PRINT}} &quot;Error:&quot;; errnum
{{Cl|RESUME}} {{Cl|NEXT}} 
{{CodeEnd}}
: ''Explanation:'' QB64 may create error 68 if COM is not found. Use a zero CD, CS, DS or OP timeout value to avoid COM timeouts!


''Example 2:'' Opening a COM port with the BIN, CS0 and DS0 options in '''QB64'''.
{{CodeStart}} '' ''
{{Cl|DIM}} bytestr {{Cl|AS}} {{Cl|STRING}} * 1  'one byte transfers
{{Cl|INPUT}} &quot;{{Cl|COM}} port number #&quot;, port$  'any COM port number available

{{Cl|OPEN}} &quot;{{Cl|COM}}&quot; + port$ + &quot;:9600,N,8,1,BIN,CS0,DS0&quot; {{Cl|FOR (file statement)|FOR}} {{Cl|RANDOM}} {{Cl|AS}} #1
{{Cl|DO}} 'main loop
    'receive data in buffer when LOC &gt; 0
    {{Cl|IF}} {{Cl|LOC}}(1) {{Cl|THEN}} 
       {{Cl|GET}} #1, , bytestr
       {{Cl|PRINT}} &quot;[&quot; + bytestr + &quot;]&quot;;
    {{Cl|END IF}}
    'transmit (send)
    k$ = {{Cl|INKEY$}}  
    {{Cl|IF}} {{Cl|LEN}}(k$) = 1 {{Cl|THEN}}
       k = {{Cl|ASC}}(k$)
       {{Cl|IF}} k &gt;= 32 {{Cl|THEN}}     'ignore control key codes
           {{Cl|PRINT}} &quot;&gt;&quot; + k$ + &quot;&lt;&quot;;
           bytestr = k$: {{Cl|PUT}} #1, , bytestr
       {{Cl|END IF}}
    {{Cl|END IF}}
{{Cl|LOOP}} {{Cl|UNTIL}} k$ = {{Cl|CHR$}}(27)
{{Cl|CLOSE}} #1: {{Cl|PRINT}} &quot;Finished!&quot; '' ''
{{CodeEnd}}


''Example 3:'' Sending string data from one COM port to another requires predefined length strings:
{{CodeStart}} '' ''
{{Cl|DIM}} {{Cl|SHARED}} ByteIn {{Cl|AS}} {{Cl|STRING}} * 1 'One byte transfers
{{Cl|DIM}} {{Cl|SHARED}} Byte4 {{Cl|AS}} {{Cl|STRING}} * 4 'Four byte transfers

Byte4 = {{Cl|CHR$}}(254) + {{Cl|CHR$}}(175) + {{Cl|CHR$}}(0) + {{Cl|CHR$}}(3) 'Command code to query all 4 banks of switch input board.

{{Cl|OPEN}} &quot;COM1:115200,N,8,1,BIN,CS0,DS0&quot; {{Cl|FOR...NEXT|FOR}} {{Cl|RANDOM}} {{Cl|AS}} #1 'Open port used to send commands.
{{Cl|OPEN}} &quot;COM2:115200,N,8,1,BIN,CS0,DS0&quot; {{Cl|FOR...NEXT|FOR}} {{Cl|RANDOM}} {{Cl|AS}} #2 'Open port used to receive commands.

{{Cl|PUT}} #1, , Byte4 'Send the 4 byte command.

Start# = {{Cl|TIMER}}
{{Cl|DO...LOOP|DO}} {{Cl|UNTIL}} {{Cl|LOC}}(2) &lt;&gt; 0 'Check if there is data received at com2
    {{Cl|IF...THEN|IF}} {{Cl|TIMER}} - Start# &gt; .5 {{Cl|THEN}} {{Cl|EXIT DO}} 'Exit loop if no data arrives within .5 seconds.
{{Cl|LOOP}}

{{Cl|IF...THEN|IF}} {{Cl|LOC}}(2) = 0 {{Cl|THEN}} 'If no data was received.....
    {{Cl|PRINT}} &quot;No data received from COM port.&quot;
    {{Cl|END}}
{{Cl|END IF}}

{{Cl|PRINT}} &quot;Received from COM2:&quot;;

{{Cl|DO...LOOP|DO}} {{Cl|UNTIL}} {{Cl|LOC}}(2) = 0 'Read data from COM2 until there is no more data.
    {{Cl|GET}} #2, , ByteIn
    {{Cl|PRINT}} {{Cl|ASC}}(ByteIn);
{{Cl|LOOP}}
{{Cl|END}} '' ''
{{CodeEnd}}{{small|Code courtesy of Hydrofoiler}}


''See also:''
* [[BINARY]], [[RANDOM]] 
* [[INPUT$]], [[PRINT (file statement)|PRINT #]]
* [[LOC]], [[INKEY$]], [[OPEN]]
* [[GET|GET #]], [[PUT|PUT #]]
* [[Port Access Libraries]] {{text|(Includes full LPT and COM port descriptions with downloadable DLL library)}}
* [[Windows_Libraries#Windows_Ports|Enumerating Windows Ports]]


{{PageNavigation}}